HAND DRIER

Special Features
•	HYGIENIC NO TOUCH OPERATION
•	VANDAL RESISTANT CASING
•	STAINLESS STEEL OR WHITE GLOSS FINISH
•	SPACE SAVING COMPACT DESIGN
•	HIGH OUTPUT HEATER AND FAN FOR FASTER DRYING
•	BRITISH SAFETY COUNCIL AND CE APPROVED

Description
The high output hand drier offers the user exceptionally fast hand drying and hygienic “No Touch” operation. Designed to he compact and space saving the drier is available with either a stainless steel cover or die cast aluminium cover with a white chip proof finish.

Construction
The hand drier cover is manufactured from either stainless steel or pressure die cast aluminium finished in a white chip proof gloss. Mounted onto the galvanised steel chassis is an infra red controlled printed circuit hoard and a high volume geometrically designed fan. The high output fan and the design of the air outlet provides high velocity warm air for fast hand drying. The heater element is provided with thermal overload protection and the fan motor is fitted with extra long life carbon bushes. An abuse control system is incorporated in the printed circuit board that automatically switches the drier off after 60 seconds if the outlet is obstructed.

Operation
The hand drier is fitted with an infra red sensor that provides hygienic no touch operation. The drier is switched on automatically when the user’s hands are placed under the air outlet. Removal of the hands switches the drier off.

Standards
The hand drier has both CE and British Safety Council approval.

Installation
The hand drier should be installed level, at the required height and securely fixed to the wall. Detailed installation instructions are supplied with the product.

Electrical Supply
220-240 VAC 50/60 Hz.

Insulation
Class 1.

Motor Speed
5500 RPM - hand drier with white cover.
2700 RPM - hand drier with stainless steel cover.

Heat Output
2.6	KW - hand drier with white cover.
1.82	KW - hand drier with stainless steel cover.

Drying Time
27 seconds - hand drier with white cover.
30 seconds - hand drier with stainless steel cover.

Operation
Infra red sensor.

Noise Level
74 dB - hand drier with white cover.
65 dB - hand drier with stainless steel cover.

Product Code Selection for Order or Quotation
1.	Base Product Code
731-hand drier with white cover
732-hand drier with stainless steel cover

As improvements in the design and performance of Acorn Powell Limited products is continuous specifications may be subject to change without notice.