Introduction
Stainless steel shower equipment is durable, vandal resistant, easy to maintain and hygienic and is suitable for use in new installations and refurbishment projects. All Acorn Powell Limited shower products are fitted with timed flow valves to conserve water and energy. As an option, thermostatically controlled manual shower valves are available on some products. Certain products in the range, like the column shower have been specifically designed to save space and installation costs. Another, the beach shower, is suitable for installing outdoors at seaside resorts. Stainless steel shower equipment is ideal for installation in leisure facilities, beach resorts, schools and educational establishments, sports stadia, factories, penal institutions, military camps, in fact all public, commercial, industrial and institutional applications. Selected products are available with a decorative coloured Enviro-Glaze finish.

Special Features
•	HYGIENIC VANDAL RESISTANT DESIGNS
•	FACTORY ASSEMBLED WITH SHOWER VALVE, SPRAY HEAD AND PIPE WORK
•	DESIGNS FOR SINGLE AND MULTIPLE USER APPLICATIONS A OPTIONAL Enviro-Glaze FINISH ON SELECTED PRODUCTS

Designs
Shower tray	Column shower	
	Available in standard or special sizes, for recess mounting or installation above floor level on to a suitable support frame. Can be used with shower panel.		Free standing, available to suit 4, 5 or 6 users. Factory fitted with all components. Shower valve and spray head for each user, individually controlled. Complete with drain anchor base. Only one water connection required.	
Shower panel				
	Surface mounted, supplied Factory fitted with all components. Panel conceals valves and pipework. Can be used with shower tray.			

Shower cubicle		Beach shower		
	Free standing open or closed top designs available in fully welded or “knockdown versions. Standard and special sizes. Factory fitted with showering components. Supplied with shower curtain, rail and soap dish.
		Free standing, available to suit 2, 3 or 4 users. Factory fitted with all components. Shower valve and spray head for each user, individually controlled. Complete with anchor base. Only one water connection required.

Installation
All shower equipment should be installed level and the edges sealed against the walls, and, if appropriate the floors, with a permanent impermeable joint.

Shower tray
Should be recessed into the floor or if required, installed above the floor on to a suitable timber or similar support frame.

Shower panel
Should be surface mounted at the required height.

Shower cubicle
Should he secured to the walls and floor. Ranges, either side by side or back to back should be bolted together on installation.

Column and Beach showers
The anchor base should be installed level into a floor recess and concreted in position. The shower column mounting flange is secured to base with the stainless steel bolts provided.

Detailed installation instructions are supplied with each product

Maintenance
Routine cleaning is necessary to maintain the appearance of stainless steel. Washing with soap or a mild detergent and warm water, applied with a sponge or bristle brush, followed by a clear water rinse is all that is required. Unless specifically formulated for use on stainless steel, bleaches, abrasive or chemical cleaners should not be used.

Earthing Continuity
All products are provided with a number of fixing points on to which an earthing continuity wire with an end terminal can be secured.

As improvements in the design and performance of Acorn Powell Limited products is continuous specifications may be subject to change without notice.