WC pans

Introduction
Stainless steel WC pans are durable, vandal resistant, easy to maintain and hygienic and are suitable for use in new installations and refurbishment projects. When calculating a project’s “whole of life cost” the use of stainless steel WC pans can offer a more economic solution than traditional ceramic or fireclay products, particularly if the installation will be prone to misuse or vandalism. Stainless steel WC pans are ideal for installation in public toilets, factories, schools and educational establishments, leisure facilities, sports stadia, entertainment venues, penal institutions, military camps, hospitals, offices, in fact all public, commercial, industrial and institutional applications. Selected WC pans are available with a coloured Enviro-Glaze finish, giving the products the appearance of ceramic, but the durability and strength of stainless steel.

Special Features
•	DURABLE AND VANDAL RESISTANT
•	ERGONOMICALLY DESIGNED
•	WATER SAVING LOW VOLUME FLUSHING
•	INTEGRAl CONTOURED SEAT WITH HIGH POLISH FINISH
•	SELF DRAINING SECURITY FLUSHING RIM
•	OPTIONAL Enviro-Glaze FINISH ON SELECTED PRODUCTS

Designs
The Acorn Powell WC pan has been specifically designed to meet the requirements of the United Kingdom and European markets. The WC pan is extremely hygienic, highly vandal resistant and has exceptional performance at low volume flushing. The elliptical shaped bowl and integral top have been ergonomically designed to provide a comfortable fully contoured seat, eliminating the need for unhygienic seat pads or a seat and cover which can be easily be damaged. The seat is highly polished to a sanitary finish and the WC pan top incorporates a security flushing rim to prevent the concealment of contriband. The WC pan complies with the constructional and performance requirements of EN 997:1999 and has been satisfactorily tested in accordance the Water Supply (water fittings) Regulations 1999:WC Suite Performance Specifications for WC suites delivering a single flush of 6 litres maximum.

Wall hung WC pan		Close coupled WC suite
		
	Designed for installing with a concealed duct mounted cistern or flush valve, the WC pan is wall hung leaving the floor clear for ease of cleaning.
		Designed for installation where ducted services are not practical, this WC suite is complete with cistern and is compact with a low overall height. The WC pan has a horizontal outlet as standard but can be converted to a vertical outlet with the addition of a WC connector A fitting kit is available to adapt the suite for use by disabled people.

	

Back to wall WC pan

Squatting WC Pan		
	Designed for installing with a concealed duct mounted cistern or flush valve. Available in two designs with either horizontal or vertical outlets.		Designed for installing level with floor surface, the WC pan has a plain vertical outlet, for connection to a suitable WC connector with integral trap.

Installation
All WC pans should be installed level and the edges sealed against the walls and floors with a permanent impermeable joint.

Wall hung WC pan
The WC pan should be secured to the wall using the bolts provided. Optional concealed WC support brackets are available.

Back to wall WC pan
The WC pan should be secured to the wall using the bolts provided and to the floor using the concealed floor fixing plate.

Close coupled WC suite
The WC suite should be secured to the wall and floor using the concealed fixing plates provided.

Squatting WC pan
The WC pan should be installed into a recess with the top edge flush with the finished floor level.

Detailed installation instructions are supplied with each product.

Maintenance
Routine cleaning is necessary to maintain the appearance of stainless steel.  Washing with soap or a mild detergent and warm water, applied with a sponge or bristle brush, followed by a clear water rinse is all that is required. Unless specifically formulated for use on stainless steel, bleaches, abrasive or chemical cleaners should not be used.

Earthing Continuity
All WC pans are provided with a number of fixing points on to which an earthing continuity wire with an end terminal can be secured.

As improvements in the design and performance of Acorn Powell Limited products is continuous specifications may be subject to change without notice.